IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
Description: "ExchangeRequirement [Architecture]"
Time stamp: "2021-06-25T20:35:05"
Originating system: "Lexocad"
Application: "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel"

People and organizations
  Person "user" "unknown" of Organization "unknown" description "organization"
  Owner history of Person "user" "unknown" of Organization "unknown" description "organization" | application "Lexocad" version "28, 0, 0, 35482" identifier "LX_SUBPRODUCTID: 2800" by Organization "Cadwork Informatik AG, CH - 4051 Basel" | change ADDED | created 1624646105 (2021-06-25T18:35:05Z) | last modified 1624646105 (2021-06-25T18:35:05Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT
  IFCSITE "Haus am See"
    IFCBUILDING "Gebäude"
      IFCBUILDINGSTOREY "EG" | elevation 0.000000000000000
        contains 12 elements
          4 x IFCWALL | type IFCWALLTYPE "Wärmedämmziegel" | STANDARD | material: "Backstein BN" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_BIMSITE, Pset_BIMsite_Links, Pset_BIMsite_Categories, Pset_ETIM
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, L10.2, lx_global
          2 x IFCANNOTATION
          2 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, L10.2, lx_global
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global
      IFCBUILDINGSTOREY "Dach" | elevation 3.800000000000000
        contains 286 elements
          232 x IFCBEAM | type IFCBEAMTYPE "Konterlattung" | object type "Konterlattung" | BEAM | names: "Dachlattung", "Konterlattung" | property sets: Qto_BeamBaseQuantities, Pset_BeamCommon, lx_global
          45 x IFCMEMBER | type IFCMEMBERTYPE "Sparren" | object type "Sparren" | names: "Pfette", "Firstpfette", "Schwelle" (+1 more) | property sets: Qto_MemberBaseQuantities, Pset_MemberCommon, lx_global
          4 x IFCPLATE | type IFCPLATETYPE "Dachfläche aussen" | object type "Dachfläche aussen" | names: "Decking", "Batten-Board" | property sets: lx_global
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Dacheindeckung" | object type "Dacheindeckung" | names: "Firstpfette" | property sets: lx_global
          2 x IFCROOF | type IFCTYPEPRODUCT "Neues Bauteil 25" | object type "Neues Bauteil 25" | names: "Dach" | property sets: lx_global
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Dacheindeckung" | names: "Ziegel" | property sets: lx_global
      IFCBUILDINGSTOREY "OG" | elevation 2.700000000000000
        contains 8 elements
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2
          4 x IFCWALL | type IFCWALLTYPE "Wärmedämmziegel" | STANDARD | material: "Backstein BN" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_DIN276, Pset_BIMsite_Categories, lx_global, Pset_ETIM
          1 x IFCSLAB | type IFCSLABTYPE "Decke" | object type "Decke" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, lx_global, L10.2
      IFCBUILDINGSTOREY "UG" | elevation -2.700000000000000
        contains 9 elements
          4 x IFCWALL | type IFCWALLTYPE "Wärmedämmziegel" | STANDARD | material: "Backstein BN" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, Pset_BIMsite_Links, Pset_BIMsite_ProductCodes, Pset_BIMsite_Documents, Pset_BIMSITE
          1 x IFCSLAB | type IFCSLABTYPE "Bodenplatte" | object type "Bodenplatte" | FLOOR | material: "Beton" | property sets: Qto_SlabBaseQuantities, Pset_SlabCommon, L10.1, lx_global
          1 x IFCSTAIR | type IFCSTAIRTYPE "Treppe" | object type "Treppe" | material: "Beton" | property sets: Pset_StairCommon, lx_global
          3 x IFCWALL | type IFCWALLTYPE "Wand 2x Typ 2" | STANDARD | material: "Beton" | property sets: Qto_WallBaseQuantities, Pset_WallCommon, lx_global, L10.2

Types
  IFCWALLTYPE "Wärmedämmziegel" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 12 occurrences | material: "Backstein BN"
  IFCWALLTYPE "Wand 2x Typ 2" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 9 occurrences | material: "Beton"
  IFCSLABTYPE "Decke" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 3 occurrences | material: "Beton"
  IFCSTAIRTYPE "Treppe" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences | material: "Beton"
  IFCBEAMTYPE "Konterlattung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 232 occurrences
  IFCMEMBERTYPE "Sparren" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 45 occurrences
  IFCPLATETYPE "Dachfläche aussen" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 4 occurrences
  IFCCOVERINGTYPE "Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence
  IFCTYPEPRODUCT "Neues Bauteil 25" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Dacheindeckung" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 2 occurrences
  IFCSLABTYPE "Bodenplatte" | element type "LX_USERDEF_COMPONENT" | USERDEFINED | 1 occurrence | material: "Beton"

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    BuildableArea = 0.000000000000000 (IFCAREAMEASURE)
    Reference = "" (IFCIDENTIFIER)
    TotalArea = 0.000000000000000 (IFCAREAMEASURE)
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 2.404321289062500
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.404321289062500
    NetVolume = 5.236803222656251
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999915519
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999915519
    NetVolume = 6.599999999788821
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.178453540802003
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.178453540802003
    NetVolume = 2.559133852004861
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.420000000014424
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.420000000014424
    NetVolume = 5.650000000036059
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.419999999954322
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.419999999954322
    NetVolume = 4.989999999885804
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 1.501546669006348
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 1.501546669006348
    NetVolume = 3.366866672515678
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 2.799999999986662
    Height = 2.500000000000000 [METRE]
    NetFootprintArea = 2.799999999986662
    NetVolume = 6.412999999966689
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    NetVolume = 6.711348553139134
  Qto_WallBaseQuantities: 12 more contents on 12 objects not shown
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 0.720000000000009
    NetArea = 0.720000000000009
    NetVolume = 0.144000000000002
    Perimeter = 3.400000000000020 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.232000000000006
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 34.078399963378942
    Perimeter = 53.000000000000000 [METRE]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.200000000000000 [METRE]
    GrossArea = 175.000000000000000
    NetArea = 175.000000000000000
    NetVolume = 35.000000000000028
    Perimeter = 53.000000000000000 [METRE]
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NosingLength = 0.000000000000000 (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 0 (IFCCOUNTMEASURE)
    NumberOfTreads = 0 (IFCCOUNTMEASURE)
    Reference = "" (IFCIDENTIFIER)
    Status in {"UNSET"} (IFCLABEL)
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104829999999994
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.011943450000005
    OuterSurfaceArea = 1.418603714262952
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000009
  Qto_BeamBaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    NetVolume = 0.011943450000004
    OuterSurfaceArea = 1.418603714262945
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000001
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.011943450000004
    OuterSurfaceArea = 1.418603714262943
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000000
  Qto_BeamBaseQuantities | quantities | on 3 objects (3 IFCBEAM)
    NetVolume = 0.017739000000000
    OuterSurfaceArea = 2.104830000000014
  Qto_BeamBaseQuantities: 158 more contents on 200 objects not shown
  Pset_BeamCommon | properties | on 232 objects (232 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  Qto_MemberBaseQuantities | quantities | on 7 objects (7 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430113
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.291999999999998
    OuterSurfaceArea = 8.799999999999965
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430078
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147812
    OuterSurfaceArea = 3.962368789400549
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149626
    OuterSurfaceArea = 3.962368789431210
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147812
    OuterSurfaceArea = 3.962368789400548
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069147812
    OuterSurfaceArea = 3.962368789400533
  Qto_MemberBaseQuantities | quantities | on 2 objects (2 IFCMEMBER)
    NetVolume = 0.094574069149559
    OuterSurfaceArea = 3.962368789430109
  Qto_MemberBaseQuantities: 23 more contents on 24 objects not shown
  Pset_MemberCommon | properties | on 45 objects (45 IFCMEMBER)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "" (IFCIDENTIFIER)
    Roll = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0.000000000000000 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"UNSET"} (IFCLABEL)
    ThermalTransmittance = 0.000000000000000 (IFCTHERMALTRANSMITTANCEMEASURE)
  lx_global | properties | on 337 objects (232 IFCBEAM, 45 IFCMEMBER, 24 IFCOPENINGELEMENT, 21 IFCWALL)
  L10.2 | properties | on 12 objects (9 IFCWALL, 3 IFCSLAB)
  Pset_ETIM | properties | on 12 objects (12 IFCWALL)
    Mit Wärmedämmung = "" (IFCLABEL)
  Pset_BIMsite_Links | properties | on 12 objects (12 IFCWALL)
    LINK_TYPE_PRODUCT_PAGE 1 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwczovL3d3dy5zY2hsYWdtYW5uLmRlL2RlL1Byb2R1a3RlL1BlcmxpdGdlZnVlbGx0ZS1aaWVnZWwvUE9ST1RPTi1TMTAiLCJjaWQiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEiLCJyaWQiOiI1MDMxMzExIiwicGlkIjoiZDViNGIxNzM2ZjJjMjUzZWM5ZGYwMzlhZTMwODkzMzVmZWNlOGMyNyIsInNpZCI6IjE2NDY5MDE5IiwidXQiOjEsImxjIjoiZGUiLCJpYXQiOjE2MjQxOTU3OTgsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEifQ.i-06BgHzuVQlgNvbGH_96nEmLpmp1wsauELGtp5RDbQ" (IFCLABEL)
    LINK_TYPE_TOOL 2 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwczovL3d3dy5zY2hsYWdtYW5uLmRlL2RlL1NlcnZpY2UvSW5mby1NYWlsLy1GdWVyLWlPUy11bmQtQW5kcm9pZCIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6NCwibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.JMI-SRKNOjlxA1IbnGc05BUaodTBYyu0P8mLEZ4sIQE" (IFCLABEL)
  Pset_BIMsite_Categories | properties | on 12 objects (12 IFCWALL)
    BIMSITESEARCH_CATEGORY = "Werkstoffe" (IFCLABEL)
    BIMSITE_CATEGORY = "Mauerwerk" (IFCLABEL)
    DIN276_CATEGORY 1 = "Innenwände" (IFCLABEL)
    DIN276_CATEGORY = "Außenwände" (IFCLABEL)
    ETIM_CATEGORY = "Ziegel" (IFCLABEL)
    HEINZEAWB_CATEGORY = "Mauersteine" (IFCLABEL)
    HEINZE_CATEGORY = "Mauer-Ziegel" (IFCLABEL)
    LIBRARY_CATEGORY 1 = "Steine" (IFCLABEL)
    LIBRARY_CATEGORY = "Steine" (IFCLABEL)
    REVIT_CATEGORY = "Wände Tragkonstruktion" (IFCLABEL)
  Pset_BIMsite_ManufacturerProperties | properties | on 12 objects (12 IFCWALL)
    Ausnutzungsfaktor im Brandfall \PG\S\afi = "Datenblatt" (IFCLABEL)
    Bedarf Ziegel (Stück/m²) = "16" (IFCLABEL)
    Charakteristischer Wert der Mauerwerksdruckfestigkeit fk (MN/m²) = "3.6" (IFCLABEL)
    Feuerwiderstandsklasse 1 = "für tragende raumabschließende Wände" (IFCLABEL)
    Gewicht (kg/Palette) = "821" (IFCLABEL)
    Korrigiertes, bewertetes Schalldämm-Maß RW, Bau, ref. inkl. beidseitigem Putz (dB) = "52.0" (IFCLABEL)
    Paletteninhalt (Stück) = "48" (IFCLABEL)
    Paletteninhalt (m² bzw. lfm) = "3.00" (IFCLABEL)
    Rechenwert der Eigenlast (kN/m²) = "8.5" (IFCLABEL)
    Verarbeitungsrichtwert (h/m²) = "0.4 bis 0.8" (IFCLABEL)
    Wasserdampfdurchlässigkeit (µ) = "µ = 5 / 10" (IFCLABEL)
  Pset_BIMsite_Documents | properties | on 12 objects (12 IFCWALL)
    DOCUMENT_USAGE_TYPE_CAD 10 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidHUiOiJodHRwczovL3d3dy5zY2hsYWdtYW5uLmRlL2RlL1NlcnZpY2UvTmV1YmF1L0NBRC1EZXRhaWxzIiwiY2lkIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIiwicmlkIjoiNTAzMTMxMSIsInBpZCI6ImQ1YjRiMTczNmYyYzI1M2VjOWRmMDM5YWUzMDg5MzM1ZmVjZThjMjciLCJzaWQiOiIxNjQ2OTAxOSIsInV0Ijo0LCJsYyI6ImRlIiwiaWF0IjoxNjI0MTk1Nzk4LCJpc3MiOiJodHRwczovL2FwaS5saXZlLmJpbS5zaXRlIiwic3ViIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIn0._rXQW1Svb0eUtM-TgAft2GTceODw688STQ8cKE7vDc4" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 1 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvREItUzEwLnBkZiIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6MSwibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.ytrsMM-uinV0ULXlmyOqMDqI4VLx-YexDRBLkDAJMyI/DB-S10.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 2 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidHUiOiJodHRwczovL3d3dy5oZWluemUuZGUvYXQtbWFuYWdlci9tYW5hZ2VyL2Zpcm1hLzE2NDY5MDE5LzQwNTc2NjM4IiwiY2lkIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIiwicmlkIjoiNTAzMTMxMSIsInBpZCI6ImQ1YjRiMTczNmYyYzI1M2VjOWRmMDM5YWUzMDg5MzM1ZmVjZThjMjciLCJzaWQiOiIxNjQ2OTAxOSIsInV0IjoxLCJsYyI6ImRlIiwiaWF0IjoxNjI0MTk1Nzk4LCJpc3MiOiJodHRwczovL2FwaS5saXZlLmJpbS5zaXRlIiwic3ViIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIn0.k2x1adOO14WZO97v9GVxjGNCng7jc-5y_qJY7aYfgs4" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 3 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvUHJlaXNsaXN0ZS5wZGYiLCJjaWQiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEiLCJyaWQiOiI1MDMxMzExIiwicGlkIjoiZDViNGIxNzM2ZjJjMjUzZWM5ZGYwMzlhZTMwODkzMzVmZWNlOGMyNyIsInNpZCI6IjE2NDY5MDE5IiwidXQiOjEsImxjIjoiZGUiLCJpYXQiOjE2MjQxOTU3OTgsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEifQ.cpi73rsC7TVnXBEXK6_lRqQZV-OudAzgS7TpAc0wFHw/Preisliste.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 4 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvUHJvZHVrdHByb2dyYW1tLnBkZiIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6MSwibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.liEJeV1VwpETiFtNHwF-BcgnZFnbc_liWDmEhh9Gybc/Produktprogramm.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 5 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvUGVybGl0ZmFtaWxpZS5wZGYiLCJjaWQiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEiLCJyaWQiOiI1MDMxMzExIiwicGlkIjoiZDViNGIxNzM2ZjJjMjUzZWM5ZGYwMzlhZTMwODkzMzVmZWNlOGMyNyIsInNpZCI6IjE2NDY5MDE5IiwidXQiOjEsImxjIjoiZGUiLCJpYXQiOjE2MjQxOTU3OTgsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiIxNDVhYjMzNi0zZGIyLTRmODUtOGU4ZC04NjljNjMxMzQwMmEifQ.xi2USVWu5miFfc7o3pt9QDqbqoWuUxI_EpnYLGhf4Gg/Perlitfamilie.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_DATASHEET 6 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvT2JqZWt0emllZ2VsLnBkZiIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6MSwibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.5GxicEcx69BpNAu8wUI1Jhsznr4l9LVfrqJQ3Obc00U/Objektziegel.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_MANUAL 8 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvVmVyYXJiZWl0dW5nc2hpbndlaXNlLnBkZiIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6MiwibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.vmOW0Ux8Sz2u87-cYPgDrtZ1sElTrZoyzymrrNjDBv8/Verarbeitungshinweise.pdf" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_MANUAL 9 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidHUiOiJodHRwczovL3d3dy55b3V0dWJlLmNvbS93YXRjaD92PXBwUTdMenJ5cGJFIiwiY2lkIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIiwicmlkIjoiNTAzMTMxMSIsInBpZCI6ImQ1YjRiMTczNmYyYzI1M2VjOWRmMDM5YWUzMDg5MzM1ZmVjZThjMjciLCJzaWQiOiIxNjQ2OTAxOSIsInV0IjoyLCJsYyI6ImRlIiwiaWF0IjoxNjI0MTk1Nzk4LCJpc3MiOiJodHRwczovL2FwaS5saXZlLmJpbS5zaXRlIiwic3ViIjoiMTQ1YWIzMzYtM2RiMi00Zjg1LThlOGQtODY5YzYzMTM0MDJhIn0.UKQB-YPQTsZ54qCvsBirPI_QVRTIcSE6G3L4Ke14QJ4" (IFCLABEL)
    DOCUMENT_USAGE_TYPE_PROOF_OF_QUALITY 7 = "https://media.live.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvc2NobGFnbWFubi1wb3JvdG9uLzgyMDA4ODUvWi0xNy0xLTEwMTctLTIwMTQwNTIyLnBkZiIsImNpZCI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSIsInJpZCI6IjUwMzEzMTEiLCJwaWQiOiJkNWI0YjE3MzZmMmMyNTNlYzlkZjAzOWFlMzA4OTMzNWZlY2U4YzI3Iiwic2lkIjoiMTY0NjkwMTkiLCJ1dCI6MywibGMiOiJkZSIsImlhdCI6MTYyNDE5NTc5OCwiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6IjE0NWFiMzM2LTNkYjItNGY4NS04ZThkLTg2OWM2MzEzNDAyYSJ9.x5Gy8iV_k5InTqfdk0cOhNjF9_aEEBBQknZ7VzmD4n8/Z-17-1-1017--20140522.pdf" (IFCLABEL)
  Pset_BIMsite_ProductCodes | properties | on 12 objects (12 IFCWALL)
    HAN = "3136110" (IFCLABEL)
  Pset_DIN276 | properties | on 12 objects (12 IFCWALL)
    Druckfestigkeit = 12.500000000000000 (IFCREAL)
  Pset_BIMSITE | properties | on 12 objects (12 IFCWALL)
    Ist System = "" (IFCLABEL)
    Ist Zubehör = "" (IFCLABEL)
    Schalldämpfend = "" (IFCLABEL)
  L10.1 | properties | on 1 object (1 IFCSLAB)